P3124FG BSP Upgrade 절차서

1. 현재 구동중인 O.S를 다시 확인 후, BSP를 Upgrade
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F3124FG# show Flash

Length- —tupe/info- CN path
3047184 1.8.4 -~ pak.ri8d
3087192 1.9.2 B pk.ris2
8 text File B cfeltxt

336 Koutes available (7344 Khytes used)

F3124FG# copy tFtp bootloader
IP address of remote host 7 192,168.1.1
Saurce File nane 7 p3k_boot .r13d
BootLoader key (Oxasbb) 7 0x3124134

TFTP::192,168.1,1//p3k_boot .r134 —-> bootloader
Procesd Cues/nol? ves

Received 165450 butes 'in 5.0 seconds

lirite to File susten.

Virited 165420 butes in 0.1 seconds
Erased 256 Kibute @ 0 —— 100/ conplete.
birited 165368 butes — 100% complete.

Bootloader uas updated.
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- BSP Image name : p3k_boot..r134
- Bootloader key 값 : 0x3124134
2. Booting시 BSP의 버전을 확인(기존 BSP 1.2.3 => 새로운 BSP 1.3.4)
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fpr 16 22151153 (1] RELOAD-REQUEST; systen reloaded by root Fron conso A
le 3

Susten is rebooting....

unmaunt. Flash File susten..dane
2oing doun, .

Frenier Boot Loader Version 1,3.4

Frocessor 1 Purple FLB 2800 revision 1.3
Core Freq 1 195 MHe

Model Nane : Fremier 3124FG

Main Menory : 64 MB

Flash Henory : 8 MB

Losding /Flash/p3k,r192 |,  conpleted
## Booting inage at 82000000 ...

Inage Nane: 1,9.2:

Inage Tupe:  MIPS Linux Kernel Inage (ezip compressed)

Data Size: 3078063 Butes = 2.9 MB

Load Address: 50100000

Entry Foint: 80265388

Verifuing Checksun .., 0K

Uncompressing Kernel Inage ... Il
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3. 최종적으로 OS와 BSP가 업그레이드 되었는지 확인.
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P3124FG# show version
Boot. Loader version : 1,3.4

F3124FG Softuare Version 1,9.2
Copuricht () 2001-2006 by Usiquess Inc.
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